# Static Call Graph for image .\Flash\Blinky.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Wed Nov 15 20:13:35 2023

### Maximum Stack Usage = 120 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

fputc ⇒ stdout_putchar ⇒ EventRecordData ⇒ EventRecordItem

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - BusFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DebugMon_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - FLASH_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - FPU_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - HardFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - MemManage_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - NMI_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - PVD_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - PendSV_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RCC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - Reset_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SDIO_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SVC_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SysTick_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f401xe.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - UsageFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - WWDG_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f401xe.o(.text)
  - fputc from retarget_io.o(.text) referenced from printf1.o(i.__0printf$1)
  - main from blinky.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  __asm___15_EventRecorder_c_e8d3082c__atomic_inc8 (Thumb, 18 bytes, Stack size 0 bytes, eventrecorder.o(.emb_text))
  [Called By]

  - >> GetContext

  __asm___15_EventRecorder_c_e8d3082c__atomic_inc32 (Thumb, 18 bytes, Stack size 0 bytes, eventrecorder.o(.emb_text))
  [Called By]

  - >> EventGetTS
  - >> EventRecordItem

  __asm___15_EventRecorder_c_e8d3082c__atomic_xch32 (Thumb, 16 bytes, Stack size 0 bytes, eventrecorder.o(.emb_text))
  [Called By]

  - >> EventGetTS

  __asm___15_EventRecorder_c_e8d3082c__LockRecord (Thumb, 34 bytes, Stack size 0 bytes, eventrecorder.o(.emb_text))
  [Called By]

  - >> EventRecordItem

  __asm___15_EventRecorder_c_e8d3082c__UnlockRecord (Thumb, 30 bytes, Stack size 0 bytes, eventrecorder.o(.emb_text))
  [Called By]

  - >> EventRecordItem

  LED_Initialize (Thumb, 78 bytes, Stack size 0 bytes, blinky.o(.text))
  [Called By]

  - >> main

  LED_On (Thumb, 22 bytes, Stack size 0 bytes, blinky.o(.text))
  [Called By]

  - >> main

  LED_Off (Thumb, 22 bytes, Stack size 0 bytes, blinky.o(.text))
  [Called By]

  - >> main

  Buttons_Initialize (Thumb, 66 bytes, Stack size 0 bytes, blinky.o(.text))
  [Called By]

  - >> main

  Buttons_GetState (Thumb, 20 bytes, Stack size 0 bytes, blinky.o(.text))
  [Called By]

  - >> main

  Delay (Thumb, 28 bytes, Stack size 0 bytes, blinky.o(.text))
  [Called By]

  - >> main

  SystemCoreClockSetHSI (Thumb, 222 bytes, Stack size 0 bytes, blinky.o(.text))
  [Called By]

  - >> main

  main (Thumb, 136 bytes, Stack size 0 bytes, blinky.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = main ⇒ EventRecorderInitialize ⇒ EventRecorderStart ⇒ EventRecordItem
  [Calls]
  - >> __2printf
  - >> SystemCoreClockUpdate
  - >> EventRecorderInitialize
  - >> EventRecordData
  - >> SystemCoreClockSetHSI
  - >> Delay
  - >> Buttons_GetState
  - >> Buttons_Initialize
  - >> LED_Off
  - >> LED_On
  - >> LED_Initialize
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  EventRecorderTimerGetCount (Thumb, 6 bytes, Stack size 0 bytes, eventrecorder.o(.text))
  [Called By]

  - >> EventGetTS

  EventRecorderTimerSetup (Thumb, 28 bytes, Stack size 0 bytes, eventrecorder.o(.text))
  [Called By]

  - >> EventRecorderInitialize

  EventRecorderTimerGetFreq (Thumb, 6 bytes, Stack size 0 bytes, eventrecorder.o(.text))
  [Called By]

  - >> EventRecorderClockUpdate
  - >> EventRecorderInitialize

  EventRecorderStart (Thumb, 44 bytes, Stack size 8 bytes, eventrecorder.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = EventRecorderStart ⇒ EventRecordItem
  [Calls]
  - >> EventGetTS
  - >> EventRecordItem
  [Called By]
  - >> EventRecorderInitialize

  EventRecorderEnable (Thumb, 88 bytes, Stack size 20 bytes, eventrecorder.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = EventRecorderEnable
  [Called By]
  - >> EventRecorderInitialize

  EventRecorderInitialize (Thumb, 300 bytes, Stack size 40 bytes, eventrecorder.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = EventRecorderInitialize ⇒ EventRecorderStart ⇒ EventRecordItem
  [Calls]
  - >> __aeabi_memclr4
  - >> EventRecorderTimerGetFreq
  - >> EventRecorderTimerSetup
  - >> EventRecorderEnable
  - >> EventRecorderStart
  - >> crc16_ccitt
  - >> EventGetTS
  - >> EventRecordItem
  [Called By]
  - >> main

  EventRecorderDisable (Thumb, 88 bytes, Stack size 20 bytes, eventrecorder.o(.text), UNUSED)

  EventRecorderStop (Thumb, 46 bytes, Stack size 8 bytes, eventrecorder.o(.text), UNUSED)
  [Calls]

  - >> EventGetTS
  - >> EventRecordItem

  EventRecorderClockUpdate (Thumb, 78 bytes, Stack size 8 bytes, eventrecorder.o(.text), UNUSED)
  [Calls]

  - >> EventRecorderTimerGetFreq
  - >> EventGetTS
  - >> EventRecordItem

  EventRecordData (Thumb, 278 bytes, Stack size 40 bytes, eventrecorder.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = EventRecordData ⇒ EventRecordItem
  [Calls]
  - >> __aeabi_memcpy
  - >> GetContext
  - >> EventCheckFilter
  - >> EventGetTS
  - >> EventRecordItem
  [Called By]
  - >> stdout_putchar
  - >> main

  EventRecord2 (Thumb, 70 bytes, Stack size 24 bytes, eventrecorder.o(.text), UNUSED)
  [Calls]

  - >> EventCheckFilter
  - >> EventGetTS
  - >> EventRecordItem

  EventRecord4 (Thumb, 118 bytes, Stack size 40 bytes, eventrecorder.o(.text), UNUSED)
  [Calls]

  - >> GetContext
  - >> EventCheckFilter
  - >> EventGetTS
  - >> EventRecordItem

  fputc (Thumb, 26 bytes, Stack size 16 bytes, retarget_io.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = fputc ⇒ stdout_putchar ⇒ EventRecordData ⇒ EventRecordItem
  [Calls]
  - >> stdout_putchar
  [Called By]
  - >> fputs
  [Address Reference Count : 1]
  - printf1.o(i.__0printf$1)

  fgetc (Thumb, 8 bytes, Stack size 0 bytes, retarget_io.o(.text), UNUSED)

  __backspace (Thumb, 8 bytes, Stack size 0 bytes, retarget_io.o(.text), UNUSED)

  abort (Thumb, 4 bytes, Stack size 0 bytes, retarget_io.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_assert

  __aeabi_assert (Thumb, 110 bytes, Stack size 16 bytes, retarget_io.o(.text), UNUSED)
  [Calls]

  - >> fputs
  - >> abort

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SystemInit (Thumb, 82 bytes, Stack size 0 bytes, system_stm32f4xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(.text)

  SystemCoreClockUpdate (Thumb, 174 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SystemCoreClockUpdate
  [Called By]
  - >> main

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> EventRecordData

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> EventRecorderInitialize

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __0printf$1 (Thumb, 22 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$1 (Thumb, 0 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf1.o(i.__0printf$1))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  fputs (Thumb, 24 bytes, Stack size 16 bytes, fputs.o(i.fputs), UNUSED)
  [Calls]

  - >> fputc
  [Called By]
  - >> __aeabi_assert

  ### Local Symbols

  EventRecordItem (Thumb, 206 bytes, Stack size 56 bytes, eventrecorder.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = EventRecordItem
  [Calls]
  - >> __asm___15_EventRecorder_c_e8d3082c__UnlockRecord
  - >> __asm___15_EventRecorder_c_e8d3082c__LockRecord
  - >> __asm___15_EventRecorder_c_e8d3082c__atomic_inc32
  [Called By]
  - >> EventRecord4
  - >> EventRecord2
  - >> EventRecorderClockUpdate
  - >> EventRecorderStop
  - >> EventRecorderStart
  - >> EventRecorderInitialize
  - >> EventRecordData

  EventGetTS (Thumb, 58 bytes, Stack size 16 bytes, eventrecorder.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = EventGetTS
  [Calls]
  - >> EventRecorderTimerGetCount
  - >> __asm___15_EventRecorder_c_e8d3082c__atomic_xch32
  - >> __asm___15_EventRecorder_c_e8d3082c__atomic_inc32
  [Called By]
  - >> EventRecord4
  - >> EventRecord2
  - >> EventRecorderClockUpdate
  - >> EventRecorderStop
  - >> EventRecorderStart
  - >> EventRecorderInitialize
  - >> EventRecordData

  EventCheckFilter (Thumb, 34 bytes, Stack size 0 bytes, eventrecorder.o(.text))
  [Called By]

  - >> EventRecord4
  - >> EventRecord2
  - >> EventRecordData

  crc16_ccitt (Thumb, 66 bytes, Stack size 12 bytes, eventrecorder.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = crc16_ccitt
  [Called By]
  - >> EventRecorderInitialize

  GetContext (Thumb, 10 bytes, Stack size 8 bytes, eventrecorder.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GetContext
  [Calls]
  - >> __asm___15_EventRecorder_c_e8d3082c__atomic_inc8
  [Called By]
  - >> EventRecord4
  - >> EventRecordData

  stdout_putchar (Thumb, 68 bytes, Stack size 8 bytes, retarget_io.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = stdout_putchar ⇒ EventRecordData ⇒ EventRecordItem
  [Calls]
  - >> EventRecordData
  [Called By]
  - >> fputc

  _printf_core (Thumb, 336 bytes, Stack size 88 bytes, printf1.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uidivmod
  [Called By]
  - >> __0printf$1

  ### Undefined Global Symbols