# Static Call Graph for image .\Objects\HAD_ASM.axf

#<CALLGRAPH># ARM Linker, 5060750: Last Updated: Thu Nov 07 13:19:15 2024

### Maximum Stack Usage = 0 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

### Functions with no stack information

- __user_initial_stackheap
- __main
- __use_two_region_memory

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - BusFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - DebugMon_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - FLASH_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - FPU_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - HardFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - MemManage_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - NMI_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - PVD_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - PendSV_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RCC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - Reset_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SDIO_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SPI4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SVC_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SysTick_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f401xe.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM3_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM4_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - TIM5_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART1_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART2_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - USART6_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - UsageFault_Handler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - WWDG_IRQHandler from startup_stm32f401xe.o(.text) referenced from startup_stm32f401xe.o(RESET)
  - __main from had_asm.o(STM32F4xx_INI) referenced from startup_stm32f401xe.o(.text)

  ### Global Symbols

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f401xe.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f401xe.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f401xe.o(.text), UNUSED, KEPT)

  __main (Thumb, 0 bytes, Stack size unknown bytes, had_asm.o(STM32F4xx_INI))

  __use_two_region_memory (Thumb, 0 bytes, Stack size unknown bytes, had_asm.o(STM32F4xx_INI), UNUSED, KEPT)

  SystemInit (Thumb, 24 bytes, Stack size 0 bytes, system_stm32f4xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f401xe.o(.text)

  ### Local Symbols

  ### Undefined Global Symbols